.
Welcome to the Lynxmotion Wiki

# MES - Power Modules

Last modified by Eric Nantel on 2021/08/06 12:35
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Table of Contents

- Description
- Features
- Specifications
  - Power Module 5V
  - Power Module 12V
- Pinout
- Dimensions & Mounting

# Description

The Lynxmotion Multirotor Erector Set (MES) Power Modules provide regulated output of 5V or 12V (depending on the module) at up to 2A. The power modules are based on the TS30042 buck converter rated at up to 95% efficiency and 1MHz fixed switching frequency. The voltage input of the 12V power module varies from 12V-40V and 6V-40V for the 5V power module. The footprint is intended for the Lynxmotion MES Power Distribution Board (PDB) but is also breadboard compatible. The modules can be identified based on which box is checked on the rear of the PCB.

# Features

- Based on TS30042 buck converter
- Up to 95% efficiency
- 1 MHz +/-10% fixed switching frequency
- Compact form factor
- Breadboard friendly
- On-board power LED

# Specifications

## Power Module 5V

- Input Voltage (IN / Vin): 6V to 40V
- Output Voltage (OUT / Vout): 5V (5.1V unloaded)
- Continuous current: 2A

## Power Module 12V

- Input Voltage (IN / Vin): 12.6V to 40V
- Output Voltage (OUT / Vout): 12V (12.1V unloaded)
- Continuous current: 2A

# Pinout

|  | IN: Input voltage (Vin)
| GND: Common ground
| OUT: Output voltage (Vout)

# Dimensions & Mounting

Tags:
Created by Eric Nantel on 2020/11/13 09:54

# Recently Visited

- MES - Power Modules
- MES - Power Distribution Board (PDB) (with modules)
- 4 DoF Robotic Arm

Copyright RobotShop 2018