.
Welcome to the Lynxmotion Wiki

# 02 - Parts

Last modified by Eric Nantel on 2022/04/06 12:48
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

A4WD3 Rover
PICTURE | NAME / DESCRIPTION | SES V1 | SES V2 | Lynxmotion SKU | RobotShop SKU |
--- | --- | --- | --- | --- | --- | ---
| A4WD3 Front / Rear Plate Plates used for the front and rear of the A4WD3 frame. Made from millet aluminum (6160), CNC milled then anodized black. Contains three general-purpose cutouts intended for lights / camera / misc. |  |  | A4WD3-FP |  |
| A4WD3 Side Plate Plates used for the sides of the A4WD3 frame. Made from millet aluminum (6160), CNC milled then anodized black. Intended to be used specifically with the 36GP-555 series of planetary gear motors. |  |  | A4WD3-SP |  |
| A4WD3 Front Small Access Plate General purpose clear plastic plate made from 1.5mm thick polycarbonate material. For use with the A4WD3 Front / Rear plate. |  |  | A4WD3-FA-S-Clear |  |
| A4WD3 Front Small Access Surrounding Plate (G10) General purpose plate made from 1.5mm thick G10 composite / glass fiber material. For use with the A4WD3 Front / Rear plate. |  |  | A4WD3-FA-S-S |  |
| A4WD3 Front Small Access Plate (G10) General purpose plate made from 1.5mm thick G10 composite / glass fiber material. For use with the A4WD3 Front / Rear plate. |  |  | A4WD3-FA-S |  |
| A4WD3 Front Large Access Plate General purpose plate made from 1.5mm thick G10 composite / glass fiber material. For use with the A4WD3 Front / Rear plate. |  |  | A4WD3-FA-L |  |
| A4WD3 Electronic Plate General purpose electronics mounting plate made from 1.5mm thick G10 composite / glass fiber material. For use inside the A4WD3. Hole pattern includes mounting for one or two Dimension Engineering Sabertooth 12A motor controllers, Raspberry Pi, Arduino Uno microcontroller and BotBoarduino microcontroller. Slots can be used for installing Velcro straps for securing a main battery and passing wires. Cutouts are available for tie wraps for cable cleanup. |  |  | A4WD3-EP |  |
| A4WD3 Top Plate General purpose top plate made from 1.5mm thick G10 composite / glass fiber material. Cutout is intended to be used with the 6" A4WD3 Hatch Gasket and hatch to allow easy, water and dust resistant access to internal components such as electronics and battery. |  |  | A4WD3-TP |  |
| A4WD3 Bottom Plate General purpose plate made from 1.5mm thick G10 composite / glass fiber material. |  |  | A4WD3-BP |  |
| A4WD3 Hatch Gasket 6" Rubber gasket created in six parts for ease of manufacturing. Intended to be used with the 6" hatch and A4WD3 top plate. |  |  | A4WD3-H-G-6IN |  |
| A4WD3 Sprocket Center Plate Center plate used on the A4WD3 sprockets (tracked version) and made from 1.5mm thick G10 composite / glass fiber material. Center mounting pattern is intended to be used with the 17mm Wheel Adapter and is compatible with the FIRST / Colson mounting pattern. |  |  | A4WD3-SPK-C |  |

Tags:
Created by Eric Nantel on 2021/10/27 11:59

# Recently Visited

- Brackets (SES)
- Nuts
- Miscellaneous
- LSS Configuration Software

Copyright RobotShop 2018