.
Welcome to the Lynxmotion Wiki

# A4WD3 Tracked

Last modified by Eric Nantel on 2024/10/21 14:51
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Table of Contents

- Description
- Features
- Specifications
- Dimensions
- Media
- User Guide
- CAD Files
- What's Included
  - All Kits
  - Autonomous Kit
  - Radio Controlled Kit

# Description

The Lynxmotion A4WD3 Rugged Rover is a general purpose mobile robotic platform. The frame is intended to be used in three configurations: 4WD; Mecanum & Tracked, and variations of each platform include without electronics (so developers can integrate their own parts); an RC version and microcontroller-based for autonomous or semi-autonomous use.

The machined aluminum frame integrates rotary seals around each motor shaft, and solid rubber cord between the frame and all panel openings, making it dust and water resistant. A large marine inspection hatch on the top panel provides easy access to internal parts as well as being able to quickly swap or recharge batteries. Aside from the internal electronics mounting plate, the platform is symmetric and can be inverted.

The rover includes four powerful 12V DC motors coupled to 51:1 all metal planetary gears. The rear shaft of each motor is equipped with a magnetic encoder which provides 12 pulses per revolution (PPR). These motors provide 4WD and allow the rover to reach a top speed of around 3m/s (120”/s) without payload.

Front and rear access panels are made of G10 composite and are intended to allow users to machine openings to add their own components, which may include a wired tether for power and control, LED or LCD feedback, a handle, or whatever else their application may need. Included are a pair of transparent polycarbonate panels which allow for an internally mounted camera and/or or LED lights for increased visibility. Additional panels are available separately.

# Features

- 4x planetary geared DC motors (12V) with rear encoders
- Machined aluminum frame with G10 composite plates
- Shaft seals & solid rubber cord for water and dust resistance
- Internal mounting plate for electronics & battery

# Specifications

A4WD3 Wheeled

- Max speed: ~1.8m/s (71in/s)
- Weight: 6.8kg (15lbs)
- Rating: Water and dust resistant
- Chassis: Aluminum frame & G10 (fiberglass) Pannels
- Tracks: Two-part injection molded sprocket with G10 center and aluminum hubs with Tracks

Motors

- Output Shaft: D-Shape 8mm
- Operating Voltage: 12VDC
- Gears: Metal planetary gear
- Unload Speed: 170RPM (±10%)
- Loaded Speed: 145RPM (±10%)
- Torque: 11.5kg.cm (9.98lb.in)
- Gear Ratio: 51:1
- Current: ≤3A

Encoder

- Operating Voltage: 5V
- Signal: Square wave AB 90 deg,
- Pulse: 12 PPR
- Frequency: 800kHz

# Dimensions

- Length: 422mm / 16.614"
- Width: 451.5mm / 17.776"
- Height: 202mm / 7.953"
- Ground clearance: 63mm / 2.48"

# Media

# User Guide

| A4WD3 Tracked Rover KIT steps: 01 - Frame Base 02 - Electronics 03 - Wiring 04 - Frame Lid 05 - Tracks 06 - Setup

# CAD Files

- A4WD3-Tracked.zip

# What's Included

## All Kits
| Rover Robots | Screws |
| 1x A4WD3-KT | 8x CPS-03 | 4x SHS-19 | 64x SHS-17 | 12x SHS-18 |
| Frame Only | 10mm x M3 Setscrew | 12mm x M12 | 10mm x M3 | 10mm x M5 |
| Washers | Tubing & Hubs | Track System | A4WD3 Parts
| 4x LW-01 | 4x A4WD3-WH | 4x A4WD3-WA | 2x A4WD3-TRK | 8x A4WD3-SPK | 4x A4WD3-SPK-C
| M12 Lock Washer | 8mm to 17mm Hex Hub | 17mm Wheel Adapter | Rubber Track | Sprocket Half | Sprocket Center
| Hex Keys |  |  |  |
| 1x HEX-1.5mm | 1x HEX-10mm |  |  |  |
| Hex Key 1.5mm | Hex Key 10mm |  |  |  |

## Autonomous Kit
| Wiring | Modules | Mot. Controllers | Batteries
| 1x WH-XT60-XT30-01 | 2x SC-01 | 1x SEA-01 | 1x BBU-01 | Sabertooth | 1x SL-LP-08
| Power Harness | Servo Cable 12" | Servo Extension Cable 6" | BotBoarduino Microcontroller | 2x12A | 4000mAh 3s LiPo Battery
| Chargers | Wiring |  |  |  |
| 1x B3AC | 1x USBC-02 |  |  |  |
| LiPo Charger | USB Mini Cable |  |  |  |

## Radio Controlled Kit
| Wiring |  | Mot. Controller | Batteries
| 1x WH-XT60-XT30-01 |  | 1x SEA-01 | 1x T8S-BT | Sabertooth | 1x SL-LP-08
| Power Harness | Servo Cable 12" | Servo Extension Cable 6" | 8 CH Remote with PPM Receiver | 2x12A | 4000mAh 3s LiPo Battery
| Chargers |  |  |  |  |
| 1x B3AC |  |  |  |  |
| LiPo Charger |  |  |  |  |

Tags:
Created by Eric Nantel on 2021/07/28 07:40

# Recently Visited

- 04 - V1 Rovers & Sumo
- SES-PRO Robotic Arm UI
- Viper Sumo Assembly Instructions
- AL5D Arm Assembly Instructions Rev. 2.1
- AL5A Arm Assembly Instructions Rev. 2.1

Copyright RobotShop 2018