.
Welcome to the Lynxmotion Wiki

# BotBoarduino Microcontroller

Last modified by Eric Nantel on 2025/03/19 14:05
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Table of Contents

- Description
- Features
- Specifications
- User Guide
- CAD Files
- BotBoarduino Microcontroller

# Description

The Lynxmotion BotBoarduino Shield-Compatible Robot Controller is mix of BotBoard II and Arduino Duemilanove for your Lynxmotion robot creation. It's perfect for controlling your small robotic projects. It has an onboard speaker, three buttons and LED's, a reset button, logic and servo power inputs, an I/O bus with 20 pins and power and ground, and a 5vdc 1.5amp regulator. Up to 15 servos can be plugged in directly.

# Features

- User Interface
- Plug and Play
- Perfect for controlling your small robotic projects
- Up to 15 servos can be plugged in directly
- USB type: Mini or Mini B (not included)

# Specifications

- 6 pins can be used for analog in
- 6 pins can be used for PWM output
- 2 pins are reserved for UART/USB
- Pin 13 has an LED connected to it

# User Guide

- BotBoarduino Manual

# CAD Files

- BBU-01.zip

  #

Tags:
Created by Eric Nantel on 2021/11/01 13:12

# Recently Visited

- BotBoarduino Microcontroller
- MES - Modular Frame
- BotBoarduino Manual
- LSS Communication Protocol
- Brackets (SES)

Copyright RobotShop 2018