.
Welcome to the Lynxmotion Wiki

# SSC-32 Servo Controller

Last modified by Eric Nantel on 2023/02/08 15:51
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Table of Contents

- Description
- Specifications
- User Guide

# Description

The SSC-32 (serial servo controller) is a small preassembled servo controller with some big features. It has high resolution (1uS) for accurate positioning, and extremely smooth moves. The range is 0.50mS to 2.50mS for a range of about 180°. The motion control can be immediate response, speed controlled, timed motion, or a combination. A unique "Group Move" allows any combination of servos to begin and end motion at the same time, even if the servos have to move different distances. This is a very powerful feature for creating complex walking gaits for multi servo walking robots. The servo's position or movement can be Queried to provide feedback to the host computer. There is even a 12 servo Hexapod sequencer built in. This allows complete control of all aspects of the alternating tripod gait simply by transferring a few values from the host controller. Any output can be used as a TTL level output. There are 4 digital inputs that are static or latched, so you don't have to worry about missing a short event. They can also be used as analog inputs. There are three terminal blocks for powering options. The DB9 input has true RS-232 levels for use with a PC.

# Specifications

These specifications pertain to firmware version 2.03XE:

- Microcontroller = Atmel ATMEGA168-20PU
- EEPROM = 24LC256P
- Speed = 14.75 MHz
- Internal Sequencer = 12 Servo Hexapod (Alternating Tripod)
- Serial input = True RS-232 or TTL, 2400, 9600, 38.4k, 115.2k, N81
- Outputs = 32 (Servo or TTL)
- Inputs = 4 (Static or Latching, Analog or Digital)
- Current requirements = 31mA
- PC interface = DB9F
- Microcontroller interface = Header posts
- Servo control = Up to 32 servos plug in directly
- Servo type supported = Futaba or Hitec
- Servo travel range = 180°
- Servo resolution = 1uS, .09°
- Servo speed resolution = 1uS / Second
- Servo motion control = Immediate, Timed, Speed or Synchronized.
- PC board size = 3.0" x 2.3"
- VS peak current = max 15 amps per side
- VS steady current = max 3-5 amps per side recommended

# User Guide

- SSC-32 Manual
- SSC-32 Firmware Downloads
- SSC-32 Binary Commands
- SSC-32 General Purpose Sequencer
- ssc32sch.pdf
- ssc-32.pdf

Tags:
Created by Eric Nantel on 2023/01/24 09:17

# Recently Visited

- SSC-32 Servo Controller

Copyright RobotShop 2018