.
Welcome to the Lynxmotion Wiki

# Wiring

Last modified by Eric Nantel on 2024/10/28 13:19
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

PICTURE | NAME / DESCRIPTION | Lynxmotion SKU | RobotShop SKU | CAD
--- | --- | --- | --- | ---
| Lynxmotion PRO CAN / Ethernet Cable Communication cables used in the Lynxmotion PRO system Lengths: 50cm, 65cm, 90cm | LSS-P-ETH-500 LSS-P-ETH-650 LSS-P-ETH-900 |  |
| Lynxmotion PRO Power XT60 Extension Cable Power cables used in the Lynxmotion PRO system Lengths: 50cm, 65cm, 90cm, 2m | LSS-P-XT60-500 LSS-P-XT60-650 LSS-P-XT60-900 |  |
| M12 to M12 Extension Cable (6') Data and power cable used for DH Robotics two and three finger grippers | CUSM128P-IOC-MF-3M | RB-2it-01 |
| Lynxmotion USB A to Type C Data and power cable Length: 1.5m or more | DH-20M50054 | RB-Sha-128 |
| Lynxmotion Smart Servo (LSS) - Serial Cables Lynxmotion SKU: 100mm / 150mm / 200mm 300mm | LSS-C-100-S LSS-C-150-S LSS-C-200-S LSS-C-300-S | RB-Lyn-999 RB-Lyn-997 RB-Lyn-995 RB-Lyn-992 |
| Lynxmotion Smart Servo (LSS) - 300mm RC Cable This cable allows the LSS servos to be easily connected to a standard 3-pin RC source. The fourth connector (from the servo's Tx pin) is separate. Should additional length be needed, a standard 3-pin servo extension (male to female) cable can be used. | LSS-C-300-RC | RB-Lyn-993 |
| Lynxmotion Smart Servo (LSS) - Serial Y Cables Lynxmotion SKU: 100mm / 150mm / 200mm / 300mm | LSS-C-100-Y LSS-C-150-Y LSS-C-200-Y LSS-C-300-Y | RB-Lyn-998 RB-Lyn-996 RB-Lyn-994 RB-Lyn-991 |
| Plastic Cable Clip Clip intended to be mounted to SES V2 brackets to help with wire routing. Magnets are meant to attach external shells. | CC-01 |  |
| Magnets for the Cable Clip Small magnet used | CC-MAG |  |
| Extra Long Stacking Headers These extra long stacking headers are intended to be use with the LSS Adapter and fit through the board. They are used to stack a shield above the LSS adapter and onto a shield compatible microcontroller. | LSS-ADA-HK | RB-Lyn-1025 |
| Lynxmotion USB A to Mini B Length: 91.44cm / 36" | USBC-02 | RB-Dfr-380 |
| Lynxmotion USB A to Type C Length: 1m / 39.37" | USBC-03 | RB-Cyt-293 |
| Servo Extender Cable 6" | SEA-01 | RB-Onl-02 |
| Servo Extender Cable 12" | SEA-02 | RB-Onl-03 |
| Servo Extension with Bare Wires 12" | SC-01 | RB-Onl-05 |
| Pin Jumper (2.54mm) | JUMPER-2.54mm |  |
| Nylon Zip Tie 7" | ZT-07in |  |
| Power Harness XT60 to XT30 1x XT60 Male 3x XT30 Female 3x XT30 Male with 30cm 16AWG cables | WH-XT60-XT30-KT | RB-Lyn-1143 |

Tags:
Created by RB1 on 2019/05/13 11:44

# Recently Visited

- LSS Radio Control (PWM)
- MES - Modular Frame
- Wiring
- Smart Servo (LSS)
- LSS Communication Protocol

Copyright RobotShop 2018