.
Welcome to the Lynxmotion Wiki

# Brackets (SES)

Last modified by Eric Nantel on 2024/04/25 17:13
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

PICTURE | NAME / DESCRIPTION | Lynxmotion SKU | RobotShop SKU | CAD
--- | --- | --- | --- | ---
SES - "C" Brackets
| Aluminum “C” Servo Bracket High quality aluminum servo bracket, available in black anodized finish. Works great with our Multi-Purpose Servo Bracket or Heavy Duty Servo Hinge sold separately. Useful for making your own arms and legs. Fits standard size servos. | ASB-03 | RB-Lyn-80 |
| Aluminum Long “C” Servo Bracket High quality, black anodized aluminum long "C" bracket works great with our Multi-Purpose Servo Bracket or Heavy Duty Servo Hinge sold separately. Useful for making your own arms and legs. Fits standard size servos. | ASB-05 | RB-Lyn-82 |
| Aluminum Short “C” Servo Bracket V1 High quality aluminum servo bracket, available in black anodized finish. Works great with our Multi-Purpose Servo Bracket or Heavy Duty Servo Hinge sold separately. Useful for making your own arms and legs with ball bearings. Fits standard sizes Hitec servos. | ASB-09 | RB-Lyn-101 |
| Aluminum Long “C” Servo Bracket V1 High quality aluminum servo bracket, available in black anodized finish. Works great with our Multi-Purpose Servo Bracket or Heavy Duty Servo Hinge sold separately. Useful for making your own arms and legs with ball bearings. Fits standard sized Hitec servos. | ASB-10 | RB-Lyn-102 |
| Aluminum Offset Servo Bracket V1 High quality aluminum servo bracket, available in black anodized finish. Works great with our Multi-Purpose Servo Bracket or Heavy Duty Servo Hinge sold separately. Useful for making your own arms and legs with ball bearings. The offset hinge was made specifically for use in Biped shoulders, but can also be used anywhere an offset is required. Fits standard size servos. | ASB-11 | RB-Lyn-103 |
| Aluminum Short “C” Servo Bracket V2 The Lynxmotion Servo Erector Set (SES) V2 Short C bracket is an evolution of the Lynxmotion ASB-09 aluminum bracket which includes the new v2 and v2b mounting patterns, as well as cutouts to pass wires and connect cable clips. | ASB-39 | RB-Lyn-1006 |
| Aluminum Long "C" Servo Bracket V2 The Lynxmotion Servo Erector Set (SES) V2 Long C bracket is an evolution of the Lynxmotion ASB-09 aluminum bracket which includes the new v2 and v2b mounting patterns, as well as cutouts to pass wires and connect cable clips. Unlike the short C bracket, the long C bracket can pass entirely around the Lynxmotion Smart Servo case. | ASB-40 | RB-Lyn-1007 |
| Aluminum Offset Servo Bracket V2 The Lynxmotion Servo Erector Set (SES) V2 Long C bracket is an evolution of the Lynxmotion ASB-09 aluminum bracket which includes the new v2 and v2b mounting patterns, as well as cutouts to pass wires and connect cable clips. Unlike the short or long C brackets, when installed on a Lynxmotion Smart Servo, the angled C bracket lines up with the servo’s case on the side. | ASB-37 | RB-Lyn-1005 |
| Aluminum Mini "C" Servo Bracket | ASB-43 | RB-Kcp-103 (ask for price & availability) |
SES - Hitec Brackets
| Aluminum E-Z Servo Bracket Here's an ingenuous way to horizontally mount standard Hitec servos that requires no screws. Made from high quality anodized aluminum "L" brackets and nylon snap rivets. It only requires you to drill some 11/64" (4.35mm) holes. Then it's a simple matter of pushing in the rivets. Literally mount servos in seconds. | ASB-02 | RB-Lyn-79 |
| Aluminum Multipurpose Servo Bracket High quality aluminum servo bracket, available in black anodized finish. Works great for making multi-axis joints for use in robot arms and legs. Fits only standard size Hitec servos. | ASB-04 | RB-Lyn-81 |
| Aluminum Inline Multi-Purpose Servo Bracket High quality aluminum servo bracket, available in black anodized finish. Works great for making multi-axis joints for use in robot arms and legs. The "inline" means that the SES patterns on the side are in line with the servo shaft. Fits standard size servos. | ASBI-04 | RB-Lyn-391 |
| Aluminum "L" Connector Bracket These high quality aluminum servo bracket, available in black anodized finish, are designed to attach a "C" bracket to the end of a Multi-Purpose servo bracket. There are several other configurations possible. Sold in a 2-pack. Material thickness is .093". | ASB-06 | RB-Lyn-83 |
| Aluminum Dual Servo Bracket (single) High quality black anodized aluminum servo bracket. Used where you need to double the servos on a single axis for increased strength. Works great for the shoulder of a robot arm. Fits standard size Hitec servos. Requires an ASB-09 or ASB-10 to connect to the servo horns. | ASB-13 | RB-Lyn-329 |
| Aluminum Servo Side-Mount Bracket This bracket is part of the Low Profile Axis. However, we're offering it separately to be used to mount a servo to anything with the Servo Erector Set hole pattern. Design to be used with the plastic low profile gear set. | ASB-14 | RB-Lyn-154 |
| Aluminum Dual Inline Multi-Purpose Servo Bracket Rev2 High quality aluminum servo bracket, available in black anodized finish. Works great for making multi-axis joints for use in robot arms and legs. Fits standard size Hitec servos. | ASB-15 | RB-Lyn-330 |
| Aluminum Servo Offset Axis Bracket High quality aluminum servo bracket, available in black anodized finish. Works great for making a wrist rotate for a robotic arm, or as a bicep rotation on a humanoid arm. Fits standard size servos. | ASB-16 | RB-Lyn-177 |
| Aluminum 15 Degree Ankle Bracket High quality black anodized aluminum 15-degree ankle servo bracket. Used in the reverse knee biped legs for the ankle joint. Designed for use with ARF-02, but can work with ARF-01 as well. Sold in a 2-pack. Fits standard size servos. | ASB-17 | RB-Lyn-357 |
| Aluminum Mechanical Advantage Bracket High quality aluminum servo bracket, available in black anodized finish. Perfect for making an indirect drive axis using the Ball Bearing Hub and other components. Fits standard size servos. | ASB-21 | RB-Lyn-390 |
| Aluminum Multi-Purpose Rotate Servo High quality aluminum servo bracket, available in black anodized finish. These brackets are similar to the ASB-04 except they have the SES hole pattern on the opposite side of the servo output shaft. This makes it possible to to make a rotation that is in line with the servo. Works great for making multi-axis joints for use in robot arms and legs. Fits Hitec standard size servos. | ASB-24 | RB-Lyn-535 |
| Aluminum Inline Multi-Purpose Rotate Servo Bracket High quality aluminum servo bracket, available in black anodized finish. These brackets are similar to the ASB-04 except they have the SES hole pattern on the opposite side of the servo output shaft. The "inline" means that the SES patterns on the bottom and side of the bracket are in line with the servo shaft. Works great for making multi-axis joints for use in robot arms and legs. Fits standard sized Hitec servos. | ASBI-24 | RB-Lyn-345 |
SES - LSS Brackets
| Aluminum SES V2 Single Wide Bracket High quality black-anodized aluminum multipurpose bracket for LSS motors can be mounted in any of six locations around the LSS motor. | ASB-28 | RB-Lyn-1003 |
| Aluminum SES V2 Double Wide Bracket High quality black-anodized aluminum multipurpose bracket for LSS motors. Can be mounted on the left or right side of the LSS motor. Includes central mounting pattern and reinforcement as compared to single wide bracket. | ASB-30 | RB-Lyn-1004 |
| Aluminum Gearbox Bracket High quality black-anodized aluminum gearbox bracket for LSS motors. Intended to be used with two 8mm ball bearings, the LSS shaft, LSS idler assembly and external gears. See sample assembly for details. | ASB-33 | RB-Kcp-92 (ask for price & availability) |
| Aluminum SES V2 Gripper Bracket Main High quality black-anodized aluminum main bracket for SES V2 system. Designed to be used with SES V2 secondary gripper bracket and gripper foam. | ASB-35 | RB-Kcp-94 (ask for price & availability) |
| Aluminum SES V2 Gripper Bracket Secondary High quality black-anodized aluminum secondary bracket for SES V2 system. Designed to be used with SES V2 main gripper bracket and gripper foam | ASB-36 | RB-Kcp-95 (ask for price & availability) |
| Foam SES V2 Gripper Bracket Foam Gripper foam. Designed to be used with SES V2 main and secondary gripper brackets. | ASB-42 | RB-Lyn-975 (ask for price & availability) |
SES - Others
| Aluminum 45 Degree Connector Bracket These high quality aluminum servo bracket, available in black anodized finish are designed to attach two brackets at a 45° angle. Material thickness is .093". | ASB-07 | RB-Lyn-327 |
| Aluminum Interconnect Bracket This high quality aluminum servo bracket, available in black anodized finish, is designed to connect two Multi-Purpose servo brackets, or for general use. | ASB-18 | RB-Lyn-180 |
| Aluminum Interconnect / Servo Horn Bracket High quality aluminum bracket, available in black anodized finish. These parts mate to the HUB-09 and the BBH-01. When used with these parts a light but very strong tubing pivot can be made. They can also be used to make a heavy duty servo horn adapter. | ASB-19 | RB-Lyn-534 |
| Aluminum Joining Bracket - 3” High quality black-anodized aluminum multi-purpose joining bracket. Works great for making larger assemblies. Connect any of the Servo Erector Set brackets, hubs, and accessories with their 2-56 hardware. Can be drilled for 3mm or 4-40 hardware. Made with .09" aluminum. | ASB-25 | RB-Lyn-331 |
| Aluminum Low Profile Axis Low Profile Axis (LPA-01) includes a brushed aluminum bracket, Acetal gears, and a Ball Bearing Hub (BBH-01). This makes a very strong pivot while only adding 0.486" to the length. It works great with all of our other brackets and hubs. Easily add waist rotate to a biped, a sixth DOF to a Biped leg, or wrist rotate to a robotic arm. This part makes many interesting and unusual mechanical assemblies possible. | LPA-01 | RB-Lyn-174 |
| Aluminum Robot Foot Rev.1 These aluminum robot feet measure 2.50" x 4.75". They have a bend on the long dimension for added strength, and some holes to lighten the foot. They will work perfectly for a humanoid biped design. Available in black anodized or brushed finish. | ARF-01 | RB-Lyn-255 |
| Aluminum Robot Foot Rev.2 These aluminum robot feet measure 3.00" x 5.00". They have a bend on the long dimension for added strength, and some holes to lighten the foot. They were designed specifically for the reverse knee leg design, but will work perfectly for a humanoid biped design as well. Available in black anodized or brushed finish. | ARF-02 | RB-Lyn-183 |
| Aluminum Black Anodized Channels High quality aluminum multi-purpose "U" channel. Available in black anodized .06" aluminum, or .09" brushed aluminum. Works great for making larger assemblies. Connect any of the Servo Erector Set brackets, hubs, and accessories with their 2-56 hardware. Can be drilled for 3mm or 4-40 hardware. Variety of different lengths available: | Choose length: 3" (ASB-503) 4" (ASB-504) 5" (ASB-505) 6" (ASB-506) 7" (ASB-507) 12" (ASB-512) 13" (ASB-513) 16" (ASB-516) | Choose length: 3" (RB-Kcp-03) 4" (RB-Kcp-04) 5" (RB-Kcp-05) 6" (RB-Kcp-06) 7" (RB-Kcp-07) 12" (RB-Kcp-08) 13" (RB-Kcp-09) 16" (RB-Kcp-10) |
| Chassis Bracket w/ Access Panel (2.5”) Currently used in the mechDOG chassis but can be used with any custom application. | GPAB-01 | RB-Kcp-104 (ask for price & availability) |
| SES-PRO Arm Base Adaptation Plate | SES-P-A-BAP | RB-Lyn-1180 |

*Not sold separately on RobotShop. For replacements, please contact RobotShop.

Tags: bracket
Created by Eric Nantel on 2019/03/21 11:45

# Recently Visited

- Brackets (SES)
- MES - Modular Frame
- LSS Configuration Software
- LSS Communication Protocol
- Lynxmotion Wiki

Copyright RobotShop 2018