.
Welcome to the Lynxmotion Wiki

# Gearing & Horns

Last modified by Eric Nantel on 2024/07/03 10:06
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

PICTURE | NAME / DESCRIPTION | Lynxmotion SKU | RobotShop SKU | CAD
--- | --- | --- | --- | ---
| Aluminum Driving Horn Aluminum driving horn has the SES V2 mounting pattern and inner 24 tooth "Hitec standard" spline. | LSS-DH | RB-Lyn-1009 |
| Aluminum SES V2 Idler Horn Aluminum idler horn has the SES V2 mounting pattern and inner bore intended to be used with a 3mm bearing. | LSS-IH | RB-Lyn-1010 |
| Aluminum SES V2 Idler / Gear Spacer Custom spacer used with idler gears or horns | LSS-FLG | RB-Fit-68 (ask for price & availability) |
| SES-V2 32 Tooth Gear Material: 3D Printed Nylon Ratio: 1:1 Compatibility: SES Pattern | SES-32T | RB-2hu-03 (ask for price & availability) |
| Plastic Low Profile Gear Set Acetal (plastic) gear set from our Low Profile Axis kit. Driving gear uses 24T spline while driven gear incorporates SES V1 pattern. Designed to be used with the aluminum servo side mount bracket. These are NOT compatible with the V2 external gears. | LPAGS-01 | RB-Lyn-368 |

Tags: gearing gear
Created by Eric Nantel on 2019/03/21 11:48

# Recently Visited

- Smart Servos (LSS)

Copyright RobotShop 2018