.
Welcome to the Lynxmotion Wiki

# 550mm 5DoF Robotic Arm

Last modified by Eric Nantel on 2024/06/28 10:13
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Table of Contents

- Description
- Specifications
- Assembly & User Guides
- Dimensions
- What's Included
- What’s Needed

# Description

- Modular, customizable & reconfigurable semi-professional arm
- Easy to use with human readable communication protocol
- High accuracy and competitive payload capacity
- 550mm horizontal extension
- 2Kg payload and ±0.1 mm accuracy
- Gripper sold separately

The Lynxmotion SES-PRO 550mm 5Dof Modular Robotic Arm Kit offers a payload of 2Kg at full extension with an accuracy of ±0.1 mm. Unlike purpose-built arms, this is designed to be modular and reconfigurable to suit the user’s application. Additional degrees of freedom can be added, and existing degrees of freedom can be reconfigured or removed. The design ensures there are no evident pinch points.

Incorporates five Lynxmotion Professional Smart Servo actuators

- Strain wave gearing
- NEMA Stepper motors
- Onboard electronics
  - Microcontroller
  - Motor controller
  - Voltage regulation
  - IMU (accel & gyro)
  - CAN communication
  - Absolute angular feedback
  - Human readable communication protocol
  - … more

# Specifications

General

- Degrees of Freedom (DoF): 5
- Payload: 2Kg (no gripper)
- Max speed (cartesian):
- Collision detection: No
- ROS 2: Coming soon

Mechanical

- Horizontal reach:
- Vertical reach:
- Joint 1: ±180°
- Joint 2: ±180°
- Joint 3: ±180°
- Joint 4: ±180°
- Joint 5: ±180°

Electrical

- Input voltage: 30V (nominal)
- Max current:
- Wall adapter: 120V - 220V
- Battery power alternative: 8 cell (8S)
- Wiring: external

Communication

- Communication method: CAN Bus
- Communication protocol: LSS-P (human readable)
- Motor: NEMA 17 & 24
- Gearing: Strain wave (aka “Harmonic drive”)
- Safety: Emergency stop button & software stop
- Joint angle: 360 (restricted by external cables)

# Assembly & User Guides

Coming Soon

# Dimensions

# What's Included

- 30V Power supply
- Cables (USB, CAT5, Power)
- Mounting hardware

Smart Servo Pro (LSS-P)
2x LSS-P-L1 | 3x LSS-P-S1 |  |  |  |
LSS-PRO Lite Actuator | LSS-PRO Standard Actuator |  |  |  |

Tubing & Hubs
4x HUB-24 | 1x CF-70x67-118 | 1x CF-70x67-143 | 1x SES-P-A-B-S |  |
70mm Tube Clamp | 118mm Carbon Fiber Tube | 143mm Carbon Fiber Tube | PRO Base for LSS-P Standard or Lite |  |

# What’s Needed

- Gripper (Lynxmotion Pro gripper suggested & Coming Soon)

Tags:
Created by Eric Nantel on 2024/06/28 10:12

# Recently Visited

- Smart Servo (LSS)
- Miscellaneous
- Johnny 5 Chassis Assembly Instructions v1.0
- LSS Specifications
- Lynxmotion Wiki

Copyright RobotShop 2018