.
Welcome to the Lynxmotion Wiki

# 900mm 5DoF Robotic Arm

Last modified by Eric Nantel on 2024/06/28 10:13
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Table of Contents

- Description
- Specifications
- Quickstart Guide / Assembly
- Dimensions
- What's Included
- What’s Needed

# Description

- Modular, customizable & reconfigurable semi-professional arm
- Easy to use with human readable communication protocol
- High accuracy and competitive payload capacity
- 900mm horizontal extension
- 3Kg payload and ±0.1 mm accuracy
- Gripper sold separately

The Lynxmotion SES-PRO 900mm 5Dof Modular Robotic Arm offers a payload of 3Kg at full extension with an accuracy of ±0.1 mm. Unlike purpose-built arms, this is designed to be modular and reconfigurable to suit the user’s application. Additional degrees of freedom can be added, and existing degrees of freedom can be reconfigured or removed. The design ensures there are no evident pinch points.

Incorporates five Lynxmotion Professional Smart Servo actuators

- Strain wave gearing
- NEMA Stepper motors
- Onboard electronics
  - Microcontroller
  - Motor controller
  - Voltage regulation
  - IMU (accel & gyro)
  - CAN communication
  - Absolute angular feedback
  - Human readable communication protocol
  - … more

# Specifications

General

- Degrees of Freedom (DoF): 5
- Payload: 3Kg (no gripper)
- Max speed (cartesian): Coming soon
- Collision detection: No
- ROS 2: Coming soon

Mechanical

- Horizontal reach: 900mm
- Vertical reach:
- Tubing material: carbon fiber
- Joint material: machined aluminum

Electrical

- Input voltage: 30V (nominal)
- Max current: Coming soon
- Wall adapter: 120V - 220V
- Battery power alternative: 8 cell (8S)
- Wiring: external

Communication

- Communication method: CAN Bus
- Communication protocol: LSS-P (human readable)
- Motor: NEMA 17 & 24
- Gearing: Strain wave (aka “Harmonic drive”)
- Safety: Emergency stop button & software stop
- Joint angle: 360 (restricted by external cables)

# Quickstart Guide / Assembly

Coming Soon

# Dimensions

# What's Included

- 30V Power supply
- Cables (USB, CAT5, Power)
- Mounting hardware

Smart Servo Pro (LSS-P)
2x LSS-P-L1 | 1x LSS-P-S1 | 2x LSS-P-M1 |  |  |
LSS-PRO Lite | LSS-PRO Standard | LSS-PRO Mega |  |  |

Tubing & Hubs
4x HUB-24 | 1x CF-70x67-280.5 | 1x CF-70x67-305.5 | 1x SES-P-A-B-S |  |
70mm Tube Clamp | 280.5mm Carbon Fiber Tube | 305.5mm Carbon Fiber Tube | PRO Base for LSS-P Standard or Lite |  |

# What’s Needed

- Gripper (Lynxmotion Pro gripper suggested & Coming Soon)

Tags:
Created by Eric Nantel on 2024/06/28 10:12

# Recently Visited

- Base Rotate
- SES-PRO Arms

Copyright RobotShop 2018