.
Welcome to the Lynxmotion Wiki

# 900mm 6DoF Zero Calibration

Last modified by Eric Nantel on 2024/10/09 07:33
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Previous
900 6DoF - Zero Calibration
Next

Disclaimer: The Lynxmotion PRO Robotic Arm is a precision tool designed for advanced users and industrial applications. This product is not a toy and should be operated with caution. Improper use may result in serious injuries. Always follow the safety guidelines and wear appropriate protective equipment when operating the robotic arm.

- 1.0 - Position the Arm
- 2.0 - Configure Temporary Offsets
- 3.0 - Move to real Zero
- 4.0 - Configure final Offsets

The Lynxmotion Smart Servo PRO (LSS-P) have multi-turn capabilities which require that an origin (zero) angle be configured for each application. In theory the origin can be anywhere between 0 and 360 degrees, but to ensure the physical arm's angles match the angular commands sent from software, a known "origin" or "zero" angle for each servo must be accurately set. Using the LSS-PRO Configuration Software and positioning the arm to a known, reproduceable position will allow for this, regardless of the "random" angle at which each joint was assembled. This requires a flat surface onto which the assembled arm can be placed.
# 1.0 - Position the Arm
| Lay the arm flat on the surface, ensuring that the servos in the elbow and wrist are fully in contact and flat against the surface as shown in the images below. This procedure can be done with or without the base plate connected, but assumes the arm's base is connected to J1. Two joints won't be constrained in this position and therefore cannot be accurately zeroed: Joint 1 (base) / ID1 and gripper (rotation) Joint 6 / ID6. It is left to the user to center these servos as needed using the procedure below.
| Side View
| Angular View
# 2.0 - Configure Temporary Offsets
| Using the LSS-PRO Configuration Software, which was already used for the LSS-PRO Configure IDs section, connect to the arm using the first actuator in the base (J1). Note: Joint 1 and 6 can be configured visually as they are not restricted by placing it on the table. Repeat the following steps for each joints
| 2.1 - Select the Joint / ID to configure
| 2.2 - In the "Custom Actions" press the "CO to Current Pos" shortcut button. This will read the current position and write it to memory as the origin, making it the new Zero degree angle.
| 2.3 - Click the Yellow "Stop & Hold" button
| 2.4 - Repeat for each Joint / ID
# 3.0 - Move to real Zero
| Now that the angle of joints 2 to 5 are known and absolute, the arm will be moved a vertical "default" position. For this, only two joints need to be moved: J2 / ID2 and J3 / ID3. As mentioned above, the known angles between J2 and J3 and J3 and J4 will differ if the SES-P Base Adaptation Plate is installed or not so be sure to use the correct angles below for your particular application / mounting. Using the "Free format command:" section of the Configuration Software move the following Joints / ID with the command provided bellow.
| 3.1 - WITHOUT Base Adaptation Plate For J2 / ID2: D9907SD500 For J3 / ID2: D907SD500 Explanation: The known angle between the shoulder (J2) and vertical 99.07 degrees. The known angle between the elbow (J3) and wrist (J5) is 9.07 degrees from aligning vertically with J2 and J3.
| 3.2 - WITH Base Adaptation Plate For J2 / ID2: D10048SD500 For J3 / ID2: D1048SD500 Explanation: The known angle between the shoulder (J2) and vertical 100.48 degrees. The known angle between the elbow (J3) and wrist (J5) is 10.48 degrees from aligning vertically with J2 and J3.
# 4.0 - Configure final Offsets
| Now that the arm is vertical, J2 and J3 origins offsets must be set to their new zero angle in this position following the same procedure as described in section "2.0 - Configure Temporary Offsets".
| 4.1 - Select the Joint / ID to configure
| 4.2 - In the "Custom Actions" press the "CO to Current Pos" shortcut button. This will read the current position and write it to memory as the origin, making it the new Zero degree angle.
| 4.3 - Click the Yellow "Stop & Hold" button
| 4.4 - Repeat for each Joint / ID

Previous
900 6DoF - Zero Calibration
Next
Tags:
Created by Eric Nantel on 2024/10/08 13:05

# Recently Visited

- LSS-PRO Configure IDs

Copyright RobotShop 2018