.
Welcome to the Lynxmotion Wiki

# SES-P Base Adaptation Plate

Last modified by Eric Nantel on 2024/07/24 14:01
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Table of Contents

- Description
- Specifications
- Dimensions
- CAD Files
- What's Included

# Description

The Lynxmotion SES-PRO Arm Base Adaptation Plate is included with each of the Lynxmotion PRO modular robotic arms, but is available separately here for customers looking for a flat and robust mounting solution for their Lynxmotion PRO project. General slots are included which are compatible with metric and imperial extrusions.

# Specifications

- Dimensions (L x W x H): 160 x 225 x 10mm
- Weight: 0.88Kg
- Compatibility: Lynxmotion small and large arm bases
- Mounting: Slots & holes for M6 or M8 screws
- Material: 6061 Aluminum

# Dimensions

# CAD Files

Main part only (SES-P-A-B-S) including Simple Geometry version:

- SES-P-A-BAP.zip

# What's Included

PICTURE | NAME / DESCRIPTION | Qty | Lynxmotion SKU | RobotShop SKU
--- | --- | --- | --- | ---
| Lynxmotion SES-PRO Arm Base Adaptation Plate | 1 | SES-P-A-BAP | RB-Jac-78 (ask for price & availability)
| Steel Socket Head Screw - Black - M4 x 12mm - 3.0mm Hex | 8 | SHS-24 | RB-Mcm-169 (ask for price & availability)
| Ball-End Hex L-Key 3.0mm | 1 | B-HEX-3.0 | RB-Mcm-202 (ask for price & availability)

NAME / DESCRIPTION

Tags:
Created by Eric Nantel on 2024/04/19 15:03

# Recently Visited

- LSS Communication Protocol
- LSS-PRO Specifications
- SES-PRO Robotic Arm UI
- A4WD3 Frame Only
- LSS-PRO Configuration Software

Copyright RobotShop 2018