.
Welcome to the Lynxmotion Wiki

# SES-P Clamp for 70mm Tubes

Last modified by Eric Nantel on 2024/07/24 14:11
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Table of Contents

- Description
- Features
- Dimensions
- CAD Files
- What's Included

# Description

The Lynxmotion SES-PRO Aluminum Clamp for 70mm CF Tubes can be mounted to both the gearbox output of any of the three Lynxmotion PRO (LSS-P) modular robotic actuators, as well as the side plate. There are several lengths of 70mm diameter Lynxmotion carbon fiber tubing compatible with this clamp. There are two variants of the Tube Clamp: a long version which includes slots for tie wraps and cable management, and a short version. The long version is included with the PRO arms.

# Features

- Lynxmotion SES-PRO Aluminum Clamp for 70mm CF Tubes
- High quality aluminum tubing connector
- Lynxmotion PRO mounting patterns
- Use with 70mm Carbon Fiber Tubing

# Dimensions

# CAD Files

Complete with all the screws

- SES-P-A-C-70-KT.zip

# What's Included

PICTURE | NAME / DESCRIPTION | Qty | Lynxmotion SKU | RobotShop SKU
--- | --- | --- | --- | ---
| Lynxmotion SES-PRO Aluminum Clamp for 70mm CF Tubes | 1 | SES-P-A-C-70 | RB-Jac-50 (ask for price & availability)
| Steel Socket Head Screw - Black - M3 x 12mm - 2.5mm Hex | 10 | SHS-22 | RB-Mcm-148 (ask for price & availability)
| Ball-End Hex L-Key 2.5mm | 1 | B-HEX-2.5 | RB-Mcm-203 (ask for price & availability)

NAME / DESCRIPTION

Tags:
Created by Eric Nantel on 2024/04/19 15:02

# Recently Visited

- Wheels
- SES-V2 - Sample Leg A
- A6WD2 Rover Assembly Guide
- Lynxmotion RIOS SSC-32: Features
- Tri-Track Tutorial for PS2 Control v1.0

Copyright RobotShop 2018