.
Welcome to the Lynxmotion Wiki

# SES-P CGE-10-10 Modular Fingers

Last modified by Eric Nantel on 2024/07/25 10:08
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Table of Contents

- Description
- Features
- Specifications
- Dimensions
- User Guides
- CAD Files
- What's Included

# Description

The Lynxmotion SES Pro fingers for the CGE-10-10 three finger gripper from DH Robotics allows for three different opening sizes for general use applications where objects being grasped are cylindrical. 120 degree jaws meet in the center when in a vertical position.

# Features

- Three mounting positions for the finger for different sized objects
- Jaw can be removed or placed in one of two configurations (vertical or horizontal)
- Anodized aluminum design
- Each finger has threaded holes on either side for 3D or 3D user-created add-ons.

# Specifications

- Specifically designed for DH Robotics’ CGE-10-10 electric three finger gripper

# Dimensions

Used on the DH-Robotics CGE-10-10 gripper (HERE)

Position 1 | Position 2 | Position 3

# User Guides

- CGE-10-10 Modular Fingers Assembly

# CAD Files

Complete with all the screws:

- SES-P-DHR-F-CGE-10-10-KT.zip

# What's Included

PICTURE | NAME / DESCRIPTION | Qty | Lynxmotion SKU | RobotShop SKU
--- | --- | --- | --- | ---
| Lynxmotion SES-PRO Finger for DHRobotics Grippers | 3 | SES-P-DHR-F | RB-Jac-97 (ask for price & availability)
| Lynxmotion SES-PRO Mounting Plate for DHRobotics CGE-10-10 Gripper | 3 | SES-P-DHR-F-CGE-10-10 | RB-Jac-96 (ask for price & availability)
| Lynxmotion SES-PRO Finger Jaw for DHRobotics Grippers | 3 | SES-P-DHR-F-J | RB-Jac-95 (ask for price & availability)
| Steel Socket Head Screw - Black - M3 x 6mm - 2.5mm Hex | 6 | SHS-30 | RB-Mcm-137 (ask for price & availability)
| Steel Socket Head Screw - Black - M4 x 8mm - 3.0mm Hex | 6 | SHS-31 | RB-Mcm-129 (ask for price & availability)
| Ball-End Hex L-Key 2.5mm | 1 | B-HEX-2.5 | RB-Mcm-203 (ask for price & availability)
| Ball-End Hex L-Key 3.0mm | 1 | B-HEX-3.0 | RB-Mcm-202 (ask for price & availability)

NAME / DESCRIPTION

Tags:
Created by Eric Nantel on 2024/05/08 11:02

# Recently Visited

- LSS Communication Protocol
- ses-v2-info (redirect)
- SES-PRO Robotic Arm UI

Copyright RobotShop 2018