.
Welcome to the Lynxmotion Wiki

# SES-P Output Shaft Cover

Last modified by Eric Nantel on 2024/07/12 12:18
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Table of Contents

- Description
- CAD Files
- What's Included

# Description

These plastic two part covers are intended to go around the gearbox section of each of the three actuators, and held in place using the Lynxmotion sleeves. The plastic simply provides lightweight spacing so the diameter of the outside of the sleeve, when mounted, corresponds to the diameter of each actuator. Holes for mounting screws to connect the two halves are provided, but the sleeve keeps the halves in place so no screws are provided. When using screws, be sure to find the appropriate size to not strip the plastic parts. If replacement covers are needed, they can be easily 3D printed without support material.

# CAD Files

- SES-P-L1-SC.zip
- SES-P-S1-SC.zip
- SES-P-M1-SC.zip

# What's Included

PICTURE | NAME / DESCRIPTION | Qty | Lynxmotion SKU |
--- | --- | --- | --- | ---
Lynxmotion SES-PRO LSS-P-L1 Output Shaft Cover Kit |  | SES-P-L1-SC-KT | RB-Lyn-1189
| Lynxmotion SES-PRO LSS-P-L1 Output Shaft Cover Half Outside Diameter: 73mm Inside Diameter: 55mm Length: 25.5mm | 2 | SES-P-L1-SC | RB-2hu-06 (ask for price & availability)
Lynxmotion SES-PRO LSS-P-S1 Output Shaft Cover Kit |  | SES-P-S1-SC-KT | RB-Lyn-1190
| Lynxmotion SES-PRO LSS-P-S1 Output Shaft Cover Half Outside Diameter: 73mm Inside Diameter: 62mm Length: 27.5mm | 2 | SES-P-S1-SC | RB-2hu-08 (ask for price & availability)
Lynxmotion SES-PRO LSS-P-M1 Output Shaft Cover Kit |  | SES-P-M1-SC-KT | RB-Lyn-1191
| Lynxmotion SES-PRO LSS-P-M1 Output Shaft Cover Half Outside Diameter: 113mm Inside Diameter: 85mm Length: 34.5mm | 2 | SES-P-M1-SC | RB-2hu-07 (ask for price & availability)

NAME / DESCRIPTION

Tags:
Created by Eric Nantel on 2024/04/30 11:31
Copyright RobotShop 2018