.
Welcome to the Lynxmotion Wiki

# SES-P DH-Robotics Control Box

Last modified by Eric Nantel on 2024/10/28 13:20
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Table of Contents

- Description
- Features
- Specifications
- Information
- CAD Files
- What's Included

# Description

The Lynxmotion SES-PRO DH Robotics USB to RS-485 Control Box is an essential component for managing the communication between USB interfaces and RS-485 used by DH-Robotics, specifically designed for seamless integration with SES-PRO robotics systems.

# Features

- Supports USB to RS-485 conversion.
- Ensures reliable data transmission.
- Compact and robust design for ease of use in various robotics applications.

# Specifications

- Input voltage: 30 to 40VDC

# Information

Front
|  | LED Indicator for Input power present.
| LED Indicator for USB connection / power present.
| M12 connector for DH-Robotics gripper systems.
| LED Indicator for Serial TX
| LED Indicator for Serial RX

Back
|  | USB Type-C connector
| XT60 power input connector (30 to 40 VDC)

# CAD Files

- USB-2DHR.zip

# What's Included

PICTURE | NAME / DESCRIPTION | Qty | Lynxmotion SKU | RobotShop SKU
--- | --- | --- | --- | ---
| Lynxmotion SES-PRO DH Robotics USB to RS-485 Control Box | 1 | USB-2DHR | (ask for price & availability)
| USB Cable A Male to C Male | 1 | DH-20M50054 | RB-Sha-128
| Lynxmotion Smart Servo PRO XT60 Female to Female Extension (90cm) | 1 | LSS-P-XT60-900 | RB-Hap-24 (ask for price & availability)
| Adhesive Rubber Feet | 4 | BS-02-BOX-TRANSPARENT | RB-Bum-01 (ask for price & availability)

NAME / DESCRIPTION

Tags:
Created by Eric Nantel on 2024/07/10 07:20

# Recently Visited

- Hex Keys
- SES-P DH-Robotics Control Box

Copyright RobotShop 2018