.
Welcome to the Lynxmotion Wiki

# 08 - Software

Last modified by Eric Nantel on 2024/10/24 07:24
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

| LSS-PRO Configuration Software The LSS PRO Config software allows a user to interface with, control, query and configure each Lynxmotion PRO smart servo motor. Command lists are provided, as well as shortcuts, a graphical output, a command line ("free command") interface, view errors and more. This software is needed to update the firmware per servo. |
| SES-PRO Robotic Arm UI The SES-PRO Robotic Arm User Interface allows customers to move the arm (joint by joint or cartesian), send and view commands and develop sequences. It includes controls for the Lynxmotion PRO Grippers (based on DH Robotics PGE-50-40 and CGE-10-10 electric grippers), sensor output and more. |
| LSS Configuration Software The Lynxmotion (LSS) - Configuration Software provides easy access to viewing and modifying of the various settings that control the main features and functionality of the Lynxmotion Smart Servo Motors as well as allowing firmware updates. |
| FlowArm LSS The Lynxmotion (LSS) - LSS FlowArm App (download) application is intended to allow easy control of the standard Lynxmotion (LSS) - 3 DoF Robotic Arm (Kit) & Lynxmotion (LSS) - 4 DoF Robotic Arm (Kit) . The graphical interface shows multiple views of the arm which can be controlled via drag and drop, as well as by manually inputting coordinates. |
| FlowArm PLTW FlowARM PLTW is a graphical interface which provides the user with complete control over the Lynxmotion AL5D robotic arm, both offline and in real time. The user is presented with multiple views of the arm, allowing the user to click and drag the arm to the desired location while the software takes care of all inverse kinematics equations. |
| FlowBotics Studio FlowBotics Studio is a development platform for robotics software: it boasts the powerful FlowBotics graphical programming language, and includes many demo robotics projects to get you started. It can be used to control just about any robotics platform, data acquisition board, motor controller, servo board, sound card, or webcam. |
| Quadrino FCT (Firmware Configuration Tool) The Quadrino FCT (Firmware Configuration Tool) is developed for the Quadrino series of flight controllers. The need for modifying the code to load the Multi-Wii on the Quadrino is eliminated by this advanced software. This high-end software offers a comprehensive solution for setting up the flight controller. |
| SSC-32 Servo Sequencer Utility The SSC-32 Servo Sequencer Utility makes it easy to control the Lynxmotion SSC-32 Servo Controller and experiment with servo-based robotics and animatronics. It also enables you to move standard R/C servo motors individually, calibrates their position, store and playback motion sequences, upgrade the SSC-32 firmware and more. |
| LynxTerm LynxTerm is a free downloadable utility, it makes it easy to quickly test all functionality of the SSC-32 Servo Controller. |

Tags: software
Created by Eric Nantel on 2022/03/16 14:20

# Recently Visited

- 06 - UAV & Drones
- MES - Folding Propeller Hub
- Quadrino Nano Drone/UAV Flight Controller (with GPS)
- MES - Power Distribution Board (PDB)
- FlowArm LSS

Copyright RobotShop 2018