.
Welcome to the Lynxmotion Wiki

# Lynx Hexapod Calibration Software

Last modified by Eric Nantel on 2023/01/25 11:17
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Table of Contents

- Description
- Download

# Description

The Hexapod Calibration program is a Flowstone based program to calibrate hexapods. This program is capable of setting the SSC-32 register offsets for all of the current Lynxmotion 3DOF Hexapods. Support for more bots coming soon!

This program is legacy and is currently not supported.

Installation Instructions:

- Download the zipped file
- Right click on the file and select 'extract all'
- Double click on the extracted 'exe' file to install

# Download

Release Date: May 31, 2012 Version: 0.1.9 Size: 2MB Download: hc120531.zip Change Log: Added support for 57600 baud rate.
Release Date: February 27, 2012 Version: 0.1.8 Size: 2MB Download: hc120227.zip Change Log: Added support for all current 3 and 4 DOF Lynxmotion hexapods. COM port scanning is more efficient and not limited by port number.
Release Date: February 2, 2012 Version: 0.0.8 Size: 2MB Download: hc120202.zip Change Log: First release.

Tags:
Created by Eric Nantel on 2023/01/25 11:02

# Recently Visited

- Lynx Hexapod Calibration Software

Copyright RobotShop 2018