.
Welcome to the Lynxmotion Wiki

# AL5C Arm

Last modified by Eric Nantel on 2024/07/03 09:21
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Table of Contents

- Description
- User Guide

# Description

About the Robot Arm The AL5C robotic arm delivers fast, accurate, and repeatable movement. The robot features: base rotation, single plane shoulder, elbow, wrist motion, a functional gripper, and optional wrist rotate. The AL5C robotic arm is an affordable system with a time tested rock solid design that will last and last. Everything needed to assemble and operate the robot is included in the kit, including RIOS, a very powerful Windows program for the SSC-32 servo controller. Note that we have tested the arm to hold at most <4oz at full reach without any additional products such as the wrist rotate upgrade installed on the arm (which decreases the payload). The lift capacity increases as the load is closer to the base, but depends on the configuration of the arm. The Mechanics The aluminum robotic arm is made from our Servo Erector Set components for the ultimate in flexibility and expandability. The kit consists of black anodized aluminum brackets, Aluminum tubing and hubs, custom injection molded components, and precision laser-cut Lexan components. The arm uses 1 x HS-475HB in the base, 1 x HS-755HB in the shoulder, 1 x HS-645MG in the elbow, 1 x HS-475HB in the wrist, and 1 x HS-422 in the gripper. The optional light weight wrist rotate uses 1 x HS-85BB. Controlling the Arm RIOS (Robotic arm Interactive Operating System) is a Windows program for controlling the AL5 series of Robotic Arms with our SSC-32 servo controller. With RIOS, your robot can be taught sequences of motion via the mouse or joystick. The inverse kinematics engine makes positioning the arm effortless. This extremely powerful program uses external digital and analog inputs to affect the robot's motion for closed loop projects. If-then, for-next, and do-while, are supported for the inputs. External outputs can also be controlled. This has been verified to work with an I/OGear USB to serial cable. If stand alone operation is desired, RIOS/SSC-32 can actually create the BASIC code to control the arm from our Bot Board and Basic Atom or Basic Stamp 2. Requires the purchase of a programming Starter Pack listed below. Note, DB9 Serial Data Cable included with AL5CC-KT. Alternately the servo motors can be controlled directly from a microcontroller. We sell the arm without servos and electronics for these options. New 3D image capture! With the addition of a GP2D12 sensor it is now possible to do experimental 3D image capturing with the latest version of RIOS. Important! To keep costs down we are not providing printed Assembly Guides. They are provided online, so you will need to print them when you order the kits. By providing the Assembly Guides online we can provide more detailed and up to date information than the old hardcopy method allowed.

# User Guide

General

- Polycarbonate Information Page
- RC Servo Mid Position Tutorial
- RC Servo Mini-Guide
- RC Digital Servo End Stops (HFP-10)

AL5C Information

- Arm Base Assembly Guide v2.1
  - Optional - Heavy Duty Metal Arm Base Assembly
- AL5C Arm Assembly Instructions Rev. 1
- Light-Weight Wrist Rotate Assembly Guide
  - Optional - Medium-Duty Wrist Rotate Assembly Guide
  - Optional - Heavy-Duty Wrist Rotate Assembly Guide
- Arm Gripper FSR Assembly Guide
  - Optional - Pneumatic Syringe Assembly Instructions
  - Optional - Vaccuum Gripper Wrist Rotate Assembly Guide
  - Optional - Gripper Assembly Instructions
- AL5 Programming Tutorial - PS2 & BotBoarduino
- Example code for AL5 arms using Arduino sketches with BotBoarduino

Additional Information

- BASIC Atom Pro Programming Tutorial
- BASIC Micro Studio Programming Tutorial for BASIC Atom Pro
- AL5 Programming Tutorial - PS2 & BotBoard II
- The Complete Hexapod 2 Tutorial
- A4WD1 & AL5 Arm Tutorial for PS2 Control
- Controlling an Arm with the Bot Board (Basic Atom) and the SSC-32
- Controlling an Arm with the Bot Board (Basic Stamp 2) and the SSC-32
- RIOS Compatible PS2 Controller to USB Adapters
- Configuring RIOS for the AL5 Series Robot Arms
- Users Manual for arms using SSC-32 and RIOS v1.06

Tags:
Created by Eric Nantel on 2024/07/03 09:20

# Recently Visited

- LSS-PRO Configuration Software
- A2WD1 Rover
- A6WD2 Rover
- Medium-Duty Wrist Rotate Assembly Guide
- medium-duty-wrist-rotate

Copyright RobotShop 2018