.
Welcome to the Lynxmotion Wiki

# LSS Button Menu

Last modified by Eric Nantel on 2024/07/12 11:23
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Important note

To revert from RC mode back to serial mode, the button menu is required. Should the button be inaccessible (or broken) when the servo is in RC mode and the user needs to change to serial mode, a 5V constant HIGH needs to be sent to the servo's Rx pin (RC PWM pin) with a common GND and wait for over 30 seconds. Normal RC PWM pulses should not exceed 2500 milliseconds. After 30 seconds, the servo will interpret this as a desired mode change and change to serial mode. This has been implemented as a fail safe.

Tags: LSS button menu navigation firmware LSS-Ref
Created by Eric Nantel on 2024/07/03 09:39

# Recently Visited

- 07 - Parts & Components
- LSS Button Menu

Copyright RobotShop 2018