.
Welcome to the Lynxmotion Wiki

# LSS Firmware Update

Last modified by Eric Nantel on 2024/07/03 09:39
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

# What's Needed

LSS - Servos | Modules | Wiring | Wiring | Wall Adapters | LSS - Config
LSS-XXX | LSS-ADA | LSS-C-XXX | USB-02 | 12V-XT60 | Config Software

LSS Configuration Software - Update Firmware
Step 1/7
1x LSS-ADA
LSS Adapter Board
Comments:Set the LSS Adapter Board to USB mode with the mode switch

LSS Configuration Software - Update Firmware
Step 2/7
1x USBC-02
USB to Mini B
1x 12V-XT60
12V w/ XT60
Comments:Connect both USB and power cables to the LSS Adapter

LSS Configuration Software - Update Firmware
Step 3/7
1x LSS-XXX
Any LSS Servo
1x LSS-C-XXX
LSS Cable
Comments:Connect the LSS cable between the LSS Adapter and the LSS. At that point you can flip the ON switch on your power supply.

LSS Configuration Software - Update Firmware
Step 4/7
LSS-Config
Configuration Soft
Comments:Open the LSS Configuration Software. Software is available HERE

LSS Configuration Software - Update Firmware
Step 5/7
LSS-Config
Configuration Soft
Comments:Select your COM port and click Connect to initiate the communication

LSS Configuration Software - Update Firmware
Step 6/7
LSS-Config
Configuration Soft
file://../../../../../../pages/lynxmotion/ses-v2/lynxmotion-smart-servo/lss-configuration-software/lss-config-firmware-update/WebHome.htmlWebHome/LSS-Config-Firmware-Button.png?=" target="_blank">

LSS Configuration Software - Update Firmware
Step 7/7
LSS-Config
Configuration Soft
file://../../../../../../pages/lynxmotion/ses-v2/lynxmotion-smart-servo/lss-configuration-software/lss-config-firmware-update/WebHome.htmlWebHome/LSS-Config-Firmware-Version.png?=" target="_blank">
Comments:The servo will now update. Wait until the process is finished in the LSS-Config.
Tags:
Created by Eric Nantel on 2024/07/03 09:39
Copyright RobotShop 2018