.
Welcome to the Lynxmotion Wiki

# LSS Electrical

Last modified by Eric Nantel on 2024/07/12 11:23
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Page Contents

- Typical Connections
- Wiring Pinout
- Electronics

# Typical Connections

In order to daisy chain one servo to the next (serial mode only), rollover serial cables are used. Although the wires are straight, one connector must be rotated 180 degrees with respect to the other.

Serial Single | Serial Multiples | Radio Control (RC) |

# Wiring Pinout

|  | Serial Mode | RC Mode
|  | Servo Rx: In serial mode, this pin should be connected to a 5V TTL serial pin. In RC mode, the pin should be connected to an 5V RC PWM pin | Servo RC Signal:Please refer to the LSS - RC PWM for more information regarding the RC mode and signals
| Servo Vcc: Refer to the Voltage section of the LSS - Specifications page to understand which voltages are meant to be connected to this pin. | Same as Serial Mode
| Ground (GND): This pin should be connected to both the communication sources' ground, as well as that of the power source (principle of "common ground"). | Same as Serial Mode
| Servo Tx: In serial mode, this pin sends the output from query commands. In RC mode, the cable does not need to be connected as there is no output. | N/A: Futur Implementation

# Electronics

|  | The electronics inside the servo include the following: H-bridge motor controller Microcontroller (Cortex M0) Magnetic position sensor Voltage sensor Temperature sensor Current sensor

Tags: LSS LSS-Ref electronics
Created by Eric Nantel on 2024/07/03 09:39

# Recently Visited

- LSS Communication Protocol

Copyright RobotShop 2018