.
Welcome to the Lynxmotion Wiki

# Geared Gripper

Last modified by Eric Nantel on 2024/07/03 09:35
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Table of Contents

- Description
- Specifications
- Assembly Guide
- What's included
- Dimensions

# Description

The Lynxmotion Servo Erector Set (SES) V2 geared gripper / pincer kit is designed to make use of the Lynxmotion Smart Servo (LSS) 's many mounting points and external modular gearing. The gripper is made of durable aluminum plates and standoffs, and uses foam to conform to the object being grasped. Inner teeth on the aluminum help "bite" into objects when necessary. Alternatively, 3D print your own inserts to customize the gripper for your robotic application.

# Specifications

- Over 180 degrees of operating angle / opening
- Aluminum frame and gears
- Compatible with Lynxmotion Smart Servos

# Assembly Guide

- LSS - Geared Gripper Assembly Guide

# What's included

SES - Mechanics
4x - ASH-20 | 9x - PHS-16 | 8x - PHS-02 | 1x - FHS-01 |  |
2x SES-32T | 1x - LSS-FLG | 2x ASB-35 | 2x ASB-36 | 4x ASB-42 |

# Dimensions

Tags:
Created by Eric Nantel on 2024/07/03 09:35

# Recently Visited

- SES-V1 3D CAD Models
- Geared Gripper
- Brackets (SES)
- LSS - Geared Gripper Assembly
- BRAT Biped SEQ Tutorial v2.01XE

Copyright RobotShop 2018