.
Welcome to the Lynxmotion Wiki

# A2WD1 Rover

Last modified by Eric Nantel on 2023/01/30 14:22
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Table of Contents

- Description
- Specifications
- User Guide

# Description

About the 2WD Servo Robot This kit can only be made as part of the Lynxmotion SES V1.1 kit and is not available separately. The Lynxmotion Aluminum 2WD Servo Robot Kit is a robust, modifiable, and expandable chassis for your RC or autonomous robot experimentation. By utilizing plastic wheels with rubber rim, robot has excellent traction. Using our small 6V NiMH battery pack and the BotBoarduino means there is plenty of room for additional sensors and electronics. The Mechanics The main robot chassis is made using Servo Erector Set modular brackets while the electronic carrier is made out of ultra-tough laser-cut Lexan. It includes two Hitec 1425CR continuous rotation servo motors and our 2.63" wheels. Controlling the Robot This version of the robot uses our Botboarduino, and comes as a bare-bones kit. You can control the basic robot via USB cable, or purchase the optional RC-01 V2 PS2 controller kit and PS2 Receiver Carrier to convert it into a remote controlled vehicle. Alternatively, you can add sensors to make it autonomous, or arduino Shields to further increase the functionality and capability. Powering Options The robot is compatible with the following batteries and chargers. Chargers & Accessories > 6.0 - 12vdc Ni-CD & Ni-MH Universal Smart Charger (USC-02) Batteries > 6.0 Volt Ni-MH 1600mAh Battery Pack (BAT-03) > 6.0 Volt Ni-MH 2800mAh Battery Pack (BAT-05) Important! To keep costs down we are not providing printed Assembly Guides. They are provided online, so you will need to print them when you order the kits. By providing the Assembly Guides online we can provide more detailed and up to date information than the old hardcopy method allowed.

# Specifications

- Servo motion control = open loop, speed control
- Steering = 2WD skid / tank
- Number of wheels = 2x driven, 1x idler (tail wheel)
- Motion speed =
- Height (overall, as in product view with BotBoarduino) = 4.5"
- Width = 6.625"
- Length = 7"
- Weight (w/out batteries) = 314g / 11oz
- Ground clearance = 0.50"

# User Guide

General

- Polycarbonate Information Page
- Motor Wiring Mini-Guide
- Wheel Encoder Assembly Guide
- Wheel & Tire Mounting
- RC Servo Mid Position Tutorial
- RC Servo Mini-Guide
- RC Digital Servo End Stops (HFP-10)

A2WD1 Rover

- A2WD1 SES Rover Assembly Guide v1.1

Tags:
Created by Eric Nantel on 2023/01/13 12:26

# Recently Visited

- A4WD1 MTS Rover
- Viper Sumo Microcontroller Instructions
- 2WD Viper Sumo v2
- Controlling an Arm with the Bot Board (Basic Atom) and the SSC-32
- Stomper Sumo Assembly Instructions v2.0

Copyright RobotShop 2018