.
Welcome to the Lynxmotion Wiki

# A4WD1 & Tri-Track RadioLink RC Control Tutorial

Last modified by Eric Nantel on 2024/08/07 14:28
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Step 1 - Sabertooth Setup
| The most important thing to set for your Sabertooth is the dip-switches that enable/disable different modes on the board. Depending on your version of the Sabertooth you will have to set the dip-switches differently so we suggest you to have a look at the different user manuals here: Sabertooth 2x5 RC Sabertooth 2x5 Sabertooth 2x12 RC Sabertooth 2x12
Step 2 - Wiring

Tags:
Created by Eric Nantel on 2023/01/30 10:55

# Recently Visited

- LSS Configuration Software
- A4WD1 & Tri-Track RadioLink RC Control Tutorial
- 07 - Parts & Components
- SES-V2 - Sample Leg A
- Smart Servo (LSS)

Copyright RobotShop 2018