.
Welcome to the Lynxmotion Wiki

# Johnny 5 Rover

Last modified by Eric Nantel on 2024/07/03 09:21
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Table of Contents

- Description
- Specifications
- User Guide

# Description

About the Johnny 5 Robot The Lynxmotion Johnny 5 Robot Kit is a very cool and completely functional model of the ever popular movie robot. The kit is available as a full Johnny 5 combo kit, or just the torso and rotating base to be added to a different style base. The robot is designed for indoor or outdoor use and performs well on many different surfaces. The Mechanics The robot is made from Servo Erector Set aluminum brackets, custom injection molded components, and ultra-tough laser-cut Lexan structural components. The torso is fully articulated utilizing 8 x HS-645MG, 3 x HS-475HB / HS-485HB, and 3 x HS-422 servos, and our SSC-32 servo controller. By utilizing heavy duty polypropylene and rubber tracks with durable ABS molded sprockets the robot has excellent traction. It includes two 12vdc 50:1 gear head motors and the Sabertooth 2 x 5 motor controller. Controlling the Robot The combo kit includes the powerful Lynxmotion Sequencer Program for PC. You can control the robot from a PC with the included DB9 cable, or use a SparkFun bluetooth modem for wireless PC control. Check out our Assembly Guides page for BlueSMiRF and SSC-32 Configuration Tutorials for specific information. Powering Options The robot is compatible with the following batteries and chargers. Accessories > NiMH Quick Connect (mates to battery) (BATC-01) > Battery Connector with Switch (WH-01) Batteries & Chargers o Servos > 6.0 Volt Ni-MH 2800mAh Battery Pack (BAT-05) o Sabertooth and Motors > 12 Volt Ni-MH 1600mAh Battery Pack (BAT-01) > 12 Volt Ni-MH 2800mAh Battery Pack (BAT-06) o Charger > 6.0 - 12vdc Universal Smart Charger (USC-02) Important! To keep costs down we are not providing printed Assembly Guides. They are provided online, so you will need to print them when you order the kits. By providing the Assembly Guides online we can provide more detailed and up to date information than the old hardcopy method allowed.

# Specifications

- Length = 10.00"
- Width = 11.00"
- Height (Overall) = 14.25"
- Height (Base and torso) = 11.75"
- Ground Clearance = 1.00"
- Deck Height = 3.00"
- Deck Dimensions = 7.25" W x 8.125" D
- Weight = 6.25 lbs (no batteries)
- Speed = 24.0 in/sec

# User Guide

General

- Polycarbonate Information Page
- Motor Wiring Mini-Guide

Johnny 5 Information

- Track Links Assembly Guide
- Johnny 5 Chassis Assembly Instructions v1.0
- Humanoid Biped Hand "A" Assembly Guide
- Johnny 5 Torso Assembly Guide
- Johnny 5 Schematic for SEQ
- Johnny 5 Schematic for Bot Board

Additional Information

- BRAT Biped SEQ Tutorial v1.06XE
- BlueSMiRF Installation Tutorial
- BlueSMiRF and SSC-32 Configuration Tutorial
- WiPort and SSC-32 Configuration Tutorial..pdf
- BASIC Atom Pro Programming Tutorial
- BASIC Micro Studio Programming Tutorial for BASIC Atom Pro

Tags:
Created by Eric Nantel on 2023/01/13 12:32

# Recently Visited

- 04 - V1 Rovers & Sumo
- Johnny 5 Rover
- FlowArm LSS
- RIOS SSC-32 Arm Control Software

Copyright RobotShop 2018