.
Welcome to the Lynxmotion Wiki

# Batteries

Last modified by Eric Nantel on 2023/06/22 06:37
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

PICTURE | NAME / DESCRIPTION | Lynxmotion SKU | RobotShop SKU | CAD
--- | --- | --- | --- | ---
| 11.1V DC, 3500mAh Lithium Ion (Li-Ion) Battery Voltage: 11.1V Number of cells: 3 Capacity: 3500 mAh Chemistry: Lithium Ion Connector: XT60 | SL-LI-01 | RB-Sta-20 (discontinued) |
| 11.1V DC, 3300mAh Lithium Ion (Li-Ion) Battery Voltage: 11.1V Number of cells: 3 Capacity: 3300 mAh Chemistry: Lithium Ion Connector: XT60 Size (excluding wiring): 70 x 55 x 19 mm / 2.75 x 2.17 x 0.75 in | SL-LI-02 | RB-Lyn-1149 |
| 11.1V DC, 4000mAh Lithium Polymer (Li-Po) Battery Voltage: 11.1V Number of cells: 3 Capacity: 4000mAh Chemistry: Lithium Polymer Connector: XT60 Size (excluding wiring): 135 x 42 x 25 mm / 5.31 x 1.65 x 0.98 in | SL-LP-08 | RB-Lyn-1150 |

Tags:
Created by RB1 on 2019/05/13 11:33

# Recently Visited

- AL5A Arm
- LSS Specifications
- LSS Configuration Software
- BRAT Biped SEQ Tutorial v2.01XE
- A4WD1 Tutorial for Autonomous Behavior v1.0

Copyright RobotShop 2018