.
Welcome to the Lynxmotion Wiki

# Miscellaneous

Last modified by Eric Nantel on 2024/06/12 11:23
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

PICTURE | NAME / DESCRIPTION | Lynxmotion SKU | RobotShop SKU | CAD
--- | --- | --- | --- | ---
| Lynxmotion Aluminum Hex Standoff Electronic Carrier | AHS-EC | RB-Lyn-1085 |
| Lynxmotion LSS Button Adapter Help reach the LSS button. | LSS-BP | (print your own) |
| Lynxmotion Knurled Knob Bore: 6mm Diameter: 25mm Thickness: 10mm Setscrew thread: 10-32 | KNB-01 | RB-Lyn-1042 |
| Lynxmotion Smart Servo (LSS) ID Sticker Sheet Number 1 to 25 Number 26 to 50 | LSS-ID-01-25 LSS-ID-26-50 | RB-2hd-01 RB-2hd-02 |
| SES compatible pen holder |  | (print your own) |
| SES compatible pen holder adapter for Bic |  | (print your own) |
| SES compatible pen holder adapter for 8mm round Pen |  | (print your own) |
| Adhesive-Back Bumpers | BRB-02 |  |
| Continuous 2mm O-Ring like material | ORING-2MM (10ft) | RB-Mcm-154 (ask for price & availability) |
| Marine grade 6" access door | A4WD3-H-6IN | RB-2sl-01 (ask for price & availability) |
| Oil Seal OD: 16mm ID: 8mm Thickness: 5mm | A4WD3-OS-16x8 | RB-2om-01 (ask for price & availability)
| Blue Thread Lock (3mL) | WBTL-1 | RB-2wb-01 (ask for price & availability) |
| Silicon Grease (3g) | WBSF-2 | RB-2wb-02 (ask for price & availability) |
| Rubber Hole Grommet Inner Diameter: 9/32" Outer Diameter: 9/16" | RHG-01 | RB-Tex-97 (ask for price & availability) |
| Rubber Hole Grommet Inner Diameter: 9/16" Outer Diameter: 1" | RHG-02 | RB-Mcm-97 (ask for price & availability) |
| Cable Tie (zip-tie) CTWR003A: small, 3" long CTWR007A: small, 7" long CT019B: large, 160mm long | CTWR003A CTWR007A CT019B | RB-Mip-01 RB-Mip-02 RB-Mip-03 (ask for price & availability) |
| Lynxmotion Velcro Clinch Strap Length: 9" / 228mm Width: 0.75" / 19mm | VCS-09 | RB-Hal-01 |

Tags:
Created by Eric Nantel on 2019/04/05 15:07

# Recently Visited

- Miscellaneous
- 04 - V1 Rovers & Sumo
- Mechanics
- Brackets (SES)
- LSS Communication Protocol

Copyright RobotShop 2018