.
Welcome to the Lynxmotion Wiki

# Nuts

Last modified by Eric Nantel on 2023/06/22 06:39
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

PICTURE | NAME / DESCRIPTION | Lynxmotion SKU | RobotShop SKU | CAD
--- | --- | --- | --- | ---
| Steel Nut Finish: Black oxide Hex: 1/4" Height / thickness: 1/16" Thread: 2-56 | SN-02 (25 pack) | RB-Lyn-247 (25pk) |
| Steel Lock Nut Finish: Chrome Hex: 1/4" Height / thickness: 9/64" Thread: 2-56 | SLN-02 | RB-Lyn-679 (25pk) |
| Steel Lock Nut Finish: Black oxide Hex: 5.5mm Height / thickness: 4mm Thread: M3 | SLN-03 | RB-Tex-117 (ask for price & availability) |
| Steel Lock Nut Finish: Black oxide Hex: 1/4" Height / thickness: 9/64" Thread: 2-56 | SLN-04 | RB-Tex-111 (ask for price & availability) |
| Steel Lock Nut Finish: Black oxide Hex: 8mm Height / thickness: 5mm Thread: M5 | SLN-05 | RB-Tex-136 (ask for price & availability) |

NAME / DESCRIPTION

Tags: SES - Nuts
Created by Eric Nantel on 2019/03/21 11:40

# Recently Visited

- A6WD2 Rover Assembly Guide
- Nuts
- 04 - V1 Rovers & Sumo
- SES-V2 - Sample Leg A
- 05 - V3 Rugged Rovers

Copyright RobotShop 2018