.
Welcome to the Lynxmotion Wiki

# Standoffs

Last modified by Eric Nantel on 2024/07/15 08:12
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

PICTURE | NAME / DESCRIPTION | Lynxmotion SKU | RobotShop SKU | CAD
--- | --- | --- | --- | ---
| Aluminum Hex Standoff (F/F) Length: 1/4" Hex: 5mm Thread: 4-40 Finish: Anodized Black | AHS-10-BA | RB-Lyn-960 (10pk) |
| Aluminum Hex Standoff (F/F) Length: 1/2" Hex: 5mm Thread: 4-40 Finish: Anodized Black | AHS-11-BA | RB-Lyn-961 (10pk) |
| Aluminum Hex Standoff (F/F) Length: 1.0" Hex: 5mm Thread: 4-40 Finish: Anodized Black | AHS-12-BA | RB-Lyn-962 (10pk) |
| Aluminum Hex Standoff (F/F) Length: 1 1/2" Hex: 5mm Thread: 4-40 Finish: Anodized Black | AHS-13-BA | RB-Lyn-963 (10pk) |
| Aluminum Hex Standoff (F/F) Length: 1 15/16" Hex: 5mm Thread: 4-40 Finish: Anodized Black | AHS-14-BA | RB-Lyn-964 (10pk) |
| Aluminum Hex Standoff (F/F) Length: 5mm Hex: 5mm Thread: M3 Finish: Anodized Black | AHS-15-BA | RB-Lyn-965 (10pk) |
| Aluminum Hex Standoff (F/F) Length: 15mm Hex: 5mm Thread: M3 Finish: Anodized Black | AHS-16-BA | RB-Lyn-966 (10pk) |
| Aluminum Hex Standoff (F/F) Length: 20mm Hex: 5mm Thread: M3 Finish: Anodized Black | AHS-17-BA | RB-Lyn-967 (10pk) |
| Aluminum Hex Standoff (F/F) Length: 25mm Hex: 5mm Thread: M3 Finish: Anodized Black | AHS-18-BA | RB-Lyn-968 (10pk) |
| Aluminum Hex Standoff (F/F) Length: 40mm Hex: 5mm Thread: M3 Finish: Anodized Black | AHS-19-BA | RB-Lyn-969 (10pk) |
| Aluminum Hex Standoff (F/F) Length: 18mm Hex: 5mm Thread: M3 Finish: Anodized Black | ASH-20-BA | RB-Lyn-970 (10pk) |
| Aluminum Hex Standoff (F/F) Length: 30mm Hex: 5mm Thread: M3 Finish: Anodized Black | ASH-21-BA | RB-Lyn-971 (10pk) |
| Aluminum Hex Standoff (F/F) Length: 10mm Hex: 5mm Thread: M3 Finish: Anodized Black | AHS-22-BA | RB-Jac-43 (ask for price & availability) |
| Aluminum Hex Standoff (F/F) Length: 10mm Hex: 5mm Thread: M3 Finish: Anodized Black | AHS-25-BA | RB-Jac-73 |
| Aluminum Hex Standoff (F/F) Length: 15mm Hex: 5mm Thread: M2.5 Finish: Anodized Black | AHS-23-BA | RB-Jac-42 (ask for price & availability) |
| Aluminum Hex Standoff (F/F) Length: 20mm Hex: 5mm Thread: M2.5 Finish: Anodized Black | AHS-24-BA | RB-Jac-41 (ask for price & availability) |
| Aluminum Hex Standoff (F/F) Length: 1 15/16" Hex: 1/4" Thread: 4-40 Finish: Aluminum Natural | AHS-02 | RB-Lyn-240 (10pk) |
| Aluminum Hex Standoff (F/F) Length: 1 1/2" Hex: 1/4" Thread: 4-40 Finish: Aluminum Natural | AHS-04 | RB-Lyn-278 (10pk) |
| Aluminum Hex Standoff (F/F) Length: 1.5" Hex: 3/16" Thread: 4-40 Finish: Aluminum Natural | AHS-06 | RB-Lyn-716 (10pk) |
| Aluminum Hex Standoff (F/F) Length: 3/16" Hex: 3/16" Thread: 4-40 Finish: Aluminum Natural | AHS-07 | RB-Lyn-721 (10pk) |
| Aluminum Hex Standoff (F/F) Length: 1/2" Hex: 3/16" Thread: 4-40 Finish: Aluminum Natural | AHS-08 | RB-Lyn-730 (10pk) |
| Aluminum Hex Standoff (F/F) Length: 1.0" Hex: 3/16" Thread: 4-40 Finish: Aluminum Natural | AHS-09 | RB-Lyn-720 (10pk) |

Tags: SES - Standoffs
Created by Eric Nantel on 2019/03/21 11:49

# Recently Visited

- LSS Communication Protocol
- Standoffs
- Smart Servos (LSS)
- SES-V2 Mounting Pattern
- Lynxmotion Wiki

Copyright RobotShop 2018