.
Welcome to the Lynxmotion Wiki

# T-Slot System

Last modified by Eric Nantel on 2023/06/22 06:40
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

PICTURE | NAME / DESCRIPTION | Lynxmotion SKU | RobotShop SKU | CAD
--- | --- | --- | --- | ---
| Aluminum T-Slot Extrusion Height: 20mm Width: 20mm Length: 100mm | AE-20-100 | RB-Lyn-951 (4pk) |
| Aluminum T-Slot Extrusion Height: 20mm Width: 80mm Length: 500mm | AE-20-500 | RB-Moa-18 |
| T-Slot Nut Threads: M4 | TNUT-M4 | RB-Lyn-944 (10pk) |
| T-Slot Swivel Nut Threads: M4 | TNUT-S-M4 | RB-Lyn-930 (10pk) |
| Aluminum Corner Connector | AE-90DEG-C | RB-Lyn-933 (4pk) |
| T-Slot Extrusion Plastic Cap (20x20) | AE-20-CAP | RB-Lyn-935 (4pk) |

NAME / DESCRIPTION

*Not sold separately on RobotShop. For replacements, please contact RobotShop.

Tags:
Created by Eric Nantel on 2020/06/30 11:26

# Recently Visited

- Controlling an Arm with the Bot Board (Basic Atom) and the SSC-32
- Wheels
- Brackets (SES)
- T-Slot System
- LSS Configuration Software

Copyright RobotShop 2018