.
Welcome to the Lynxmotion Wiki

# SES-P 70mm Carbon Fiber Tubes

Last modified by Eric Nantel on 2024/07/10 11:13
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Table of Contents

- Description
- Features
- CAD Files
- What's Included

# Description

The Lynxmotion SES-PRO 305.5mm x 70mm Carbon Fiber Tube is strong and lightweight designed to be used with Lynxmotion’s Professional Servo Erector Set (SES-Pro) aluminum clamp. Various different lengths are offered, and custom lengths can be requested.

# Features

- 70mm diameter long carbon fiber tube
- Various standard lengths of 118mm, 143mm, 280.5mm, 305.5mm
- Strong and lightweight
- Designed for Lynxmotion SES-PRO & PRO clamp

# CAD Files

- Main part & including Simple Geometry version:
  - CF-70x67-118.zip
  - CF-70x67-143.zip
  - CF-70x67-280.5.zip
  - CF-70x67-305.5.zip

# What's Included

PICTURE | NAME / DESCRIPTION | Qty | Lynxmotion SKU | RobotShop SKU
--- | --- | --- | --- | ---
| Lynxmotion SES-PRO 118mm x 70mm Carbon Fiber Tube Outside diameter: 70mm Inside diameter: 67mm Length: 118mm | 1 | CF-70x67-118-KT | RB-Lyn-1165
| Lynxmotion SES-PRO 143mm x 70mm Carbon Fiber Tube Outside diameter: 70mm Inside diameter: 67mm Length: 143mm | 1 | CF-70x67-143-KT | RB-Lyn-1166
| Lynxmotion SES-PRO 280.5mm x 70mm Carbon Fiber Tube Outside diameter: 70mm Inside diameter: 67mm Length: 280.5mm | 1 | CF-70x67-280.5-KT | RB-Lyn-1167
| Lynxmotion SES-PRO 305.5mm x 70mm Carbon Fiber Tube Outside diameter: 70mm Inside diameter: 67mm Length: 305.5mm | 1 | CF-70x67-305.5-KT | RB-Lyn-1168

NAME / DESCRIPTION

Tags:
Created by Eric Nantel on 2024/06/25 11:35

# Recently Visited

- LynxTerm
- A6WD2 Rover Assembly Guide
- LSS FlowArm - Setup
- RC Servo Mini-Guide
- Smart Servo Pro (LSS-P)

Copyright RobotShop 2018