.
Welcome to the Lynxmotion Wiki

# SES-P Arm Base for Mega

Last modified by Eric Nantel on 2024/07/22 07:52
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Table of Contents

- Description
- Features
- Dimensions
- CAD Files
- What's Included

# Description

The Lynxmotion SES-PRO Base for Mega LSS-P Actuators is intended to be used with the LSS-P-M1 professional actuator. Although the potential uses are up to the customer, the base was designed as the base for the Lynxmotion 900mm PRO modular robotic arm, or as the rotating top to a base rotation unit.

# Features

- Mount for Lynxmotion LSS-P-M1 Professional Actuator
- Milled T-6061 aluminum, anodized black

# Dimensions

# CAD Files

- Complete with all the screws:
  - SES-P-A-B-L-KT.zip
- Main part only (SES-P-A-B-L) including Simple Geometry version:
  - SES-P-A-B-L.zip
- Drilling template for the mounting holes
  - SES-P-A-B-L - Drill Template v1.0.pdf

# What's Included

PICTURE | NAME / DESCRIPTION | Qty | Lynxmotion SKU | RobotShop SKU
--- | --- | --- | --- | ---
| Lynxmotion SES-PRO Base For Mega LSS-P Actuators | 1 | SES-P-A-B-L | RB-Jac-59 (ask for price & availability)
| Steel Socket Head Screw - Black - M4 x 12mm - 3.0mm Hex | 8 | SHS-24 | RB-Mcm-169 (ask for price & availability)
| Steel Flat Head Screw - Black - M8 x 16mm - 5.0mm Hex | 4 | FHS-03 | RB-Mcm-172 (ask for price & availability)
| Ball-End Hex L-Key 3.0mm | 1 | B-HEX-3.0 | RB-Mcm-202 (ask for price & availability)
| Ball-End Hex L-Key 5.0mm | 1 | B-HEX-5.0 | RB-Mcm-196 (ask for price & availability)

NAME / DESCRIPTION

Tags:
Created by Eric Nantel on 2024/04/19 15:05

# Recently Visited

- Brackets (SES)
- Mechanics
- LSS Configuration Software
- LSS Communication Protocol
- Smart Servo (LSS)

Copyright RobotShop 2018