.
Welcome to the Lynxmotion Wiki

# SES-P T-Frame Coupler

Last modified by Eric Nantel on 2024/07/25 07:48
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Table of Contents

- Description
- Features
- Dimensions
- User Guides
- CAD Files
- What's Included

# Description

The Lynxmotion Smart Servo PRO Standard Modular T-Frame Coupler is part of the Servo Erector Set Pro (SES-PRO) modular robotic construction system. It has mounting patterns on three sides, to which all three PRO servos, the tubing clamp and other accessories can be connected. Hardware needed is included with the PRO servos or other accessories.

This is what is used to reduce the number of degrees of freedom of the 6DoF arms to 5DoF by replacing the servo in joint 4 with this fixed coupler. Similarly, J6 in the robot arm can be replaced with this coupler to further reduce it to a four degree of freedom arm. The design also reduces the weight of the servo it replaces, which improves the payload capacity.

# Features

- T-Frame coupler for use with Lynxmotion SES-PRO System
- Acts as fixed “dummy” joint in Lynxmotion PRO arms
- Durable aluminum construction

# Dimensions

# User Guides

- T-Frame Coupler Assembly

# CAD Files

Complete with all the screws including Simple Geometry version:

- LSS-P-S1-TC-KT.zip

# What's Included

PICTURE | NAME / DESCRIPTION | Quantity | Lynxmotion SKU | RobotShop SKU
--- | --- | --- | --- | ---
| Lynxmotion PRO Standard Frame | 1 | LSS-P-S1-F | RB-Jac-52 (ask for price & availability)
| Lynxmotion PRO LSS-P-S1 & L1 Frame Plate | 2 | LSS-P-S1-FP | RB-Jac-54 (ask for price & availability)
| Lynxmotion PRO LSS-P-S1 & L1 Gearbox Plate | 1 | LSS-P-S1-GP | RB-Jac-76 (ask for price & availability)
| Steel Flat Head Screw - Black - M4 x 8mm - 2.0mm Hex | 6 | FHS-07 | RB-Mcm-207 (ask for price & availability)
| Steel Socket Head Screw - Black - M3 x 8mm - 2.5mm Hex | 12 | SHS-21 | RB-Mcm-131 (ask for price & availability)
| Ball-End Hex L-Key 2.0mm | 1 | B-HEX-2.0 | RB-Mcm-198 (ask for price & availability)
| Ball-End Hex L-Key 2.5mm | 1 | B-HEX-2.5 | RB-Mcm-203 (ask for price & availability)

NAME / DESCRIPTION

Tags:
Created by Eric Nantel on 2024/04/22 09:47

# Recently Visited

- SES-P T-Frame Coupler
- T-Frame Coupler Assembly
- SES-P Output Shaft Cover

Copyright RobotShop 2018