.
Welcome to the Lynxmotion Wiki

# Heavy Duty Metal Arm Base

Last modified by Eric Nantel on 2024/07/03 09:21
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

Table of Contents

- Description

# Description

The Lynxmotion Heavy Duty Metal Arm Base (no servo) provides the ultimate in strength and rigidity. It is made from 0.093'' thick aluminum with a black anodized finish. The base can be mounted on plywood as a base for an arm, or onto other SES parts for custom builds. The compact size increases the versitility of this assembly. This kit does not include servos.

User Guide

- Heavy Duty Metal Arm Base Assembly

Tags:
Created by Eric Nantel on 2024/07/03 09:21

# Recently Visited

- 3DoF Lexan C Leg Assembly Instructions
- 09 - Support
- LSS Communication Protocol
- Hex Keys
- LSS-P - Arduino Custom Firmware

Copyright RobotShop 2018