.
Welcome to the Lynxmotion Wiki

# SES-V2 Modules

Last modified by Eric Nantel on 2024/07/03 10:05
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all / none

Export as HTML

The Servo Erector Set (SES) v2 modular building system includes a variety of electronic and electro-mechanical modules. Modules tend to have the same basic features:

- LSS connector (Molex 0099990988) with Vin, GND, Rx and Tx so they can be added to an LSS bus and daisy chained.
- Same footprint to be mountable around an LSS servo, or to LSS compatible mounting points

Mounting

Sample Wiring / Use

The section below (click to expand) provides a list of all modules and more information about each module.

Modules (click to expand)

PICTURE | NAME / DESCRIPTION | Lynxmotion SKU | RobotShop SKU | CAD
--- | --- | --- | --- | ---
| BotBoarduino Microcontroller (Arduino Compatible) Arduino & Shield compatible microcontroller board. BotBoarduino Microcontroller | BBU-01 | RB-Lyn-363 |
| SSC-32U USB Servo Controller The SSC-32U USB servo controller is a dedicated RC servo controller with some big features. It has high resolution (1uS) for accurate positioning, and extremely smooth moves. SSC-32U USB Servo Controller | SSC-32U | RB-Lyn-850 |
| LSS Adapter (Type-C) LSS-ADA Board (Type-C) | LSS-ADA-V1.1 | RB-Lyn-1116 |
| LSS Adapter (USB Mini) LSS-ADA Board (USB Mini) | LSS-ADA-V1.0 | (discontinued) |
| LSS 2IO Board Microcontroller (Arduino Compatible) LSS-2IO Board | LSS-2IO | RB-Lyn-1050 |
| LSS 2MC Board Microcontroller (Arduino Compatible) LSS-2MC Board | LSS-2MC | RB-Lyn-1110 |
| LSS 5VR Board LSS - 5VR Board | LSS-5VR | RB-Lyn-1052 |
| LSS Power Hub LSS-HUB Board | LSS-HUB | RB-Lyn-1019 |
| LSS LED Board High output single white LED LSS-LED Board | LSS-LED | RB-Lyn-1140 |
| A4WD3-LED Board High output single CREE white LED Array of 8 red LED A4WD3-LED Board | A4WD3-LED | RB-Lyn-1153 |
Discontinued
| SSC-32 Servo Controller (DB9) The SSC-32 (serial servo controller) is a small preassembled servo controller with some big features. It has high resolution (1uS) for accurate positioning, and extremely smooth moves. SSC-32 Servo Controller | SSC-32 | RB-Lyn-100 |

Tags:
Created by Eric Nantel on 2024/07/03 10:05

# Recently Visited

- SES-V2 Modules
- SES-V2 Bracket
- A4WD3-LED Board

Copyright RobotShop 2018